Substraction(16-Bit numbers):

.model small

.data

num1 dw 9999h

num2 dw 4567h

diff dw ?

.code

main proc

mov dx,data

mov ds,dx

mov ax,num1

mov bx,num2

sub ax,bx

mov diff,ax

mov ah,4ch

int 21h

endp

end main