Substraction(8-Bit numbers):

.model small

.stack 100

.data

num1 db 7

num2 db 3

diff db ?

.code

main proc

mov ax,@data

mov ds,ax

mov al,num1

mov bl,num2

sub al,bl

mov diff,al

mov ah,4ch

int 21h

endp

end main